{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"merged":[[0,0,0,7],[1,0,1,1],[1,3,1,5],[3,0,3,6],[3,7,6,7],[4,0,12,0],[4,2,6,2],[7,2,8,2],[7,7,8,7],[9,2,10,2],[9,7,10,7],[11,2,12,2],[13,0,13,5],[15,0,15,5],[18,0,18,5],[20,0,20,5],[22,1,22,5],[23,1,23,7],[24,0,24,7]]}
["门窗维修更换、背水箱更换、晾衣杆绳安装及防水处理报价表"]
["公司名称（印章）：",null,null,"联系人及电话："]
["序号","项目名称","工作内容及参数","单位","报价数量","单价（元）","合价（元）","备注"]
["一、门窗维修更换"]
[1,"拉手更换","工作内容：拉手、锁体、锁芯维修更换；                              参数：双向拉手门锁的装配，锁体锁芯安装中心线一致，锁芯长度75mm。","把",50]
[null,"锁体更换",null,"把",50]
[null,"锁芯更换",null,"把",50]
[null,"卫生间铝合金门维修","工作内容：校正、更换合页拉手，铝材维修、加固；                                               参数：铝材材质，1.0mm厚","樘",40]
[null,"阳台铝合金门维修",null,"樘",40]
[null,"卫生间隔断门维修","参数：卫生间隔断门材质PVC复合防潮板厚度3.1mm","樘",40]
[null,"卫生间隔断门更换",null,"樘",40]
[null,"室外变压器房门维修","工作内容：维修更换，线路整理；                                    参数：配电箱500*400,箱钢板厚度不低于1.2mm。","个",10]
[null,"室外配电箱更换",null,"个",10]
["二、学生宿舍1号、2号、3号、4号、5号、6号楼寝室卫生间背水箱更换安装"]
[2,"背水箱更换","工作内容：拆除原有脚踏冲水阀及凿开地面，安装PPR25管及PPR25内丝弯头，并用混凝土恢复地面、墙面背水箱管道处，卫生清运。                                           参数：塑料水箱，PE材质，容量6升，进水流量≥0.05L/S，动压力0.5MPa下，进水阀闭密封密，无渗透现象，进水阀抗热性，无渗漏变形，进水阀水机≤0.2MPa，进水噪声≤55dB，排水阀密封性可自动关闭复位，且无渗漏现象，排水阀密封件耐腐蚀性，重量变化≤1g或5%，尺寸变化 ≤1mm或5%，排水流量≥1.7L/s，含三角阀、金属软管等配件；                                      ","套",600]
["三、不锈钢晾衣杆、绳安装"]
[3,"不锈钢绳安装","工作内容：人工安装； 参数：规格7*19，材质304，直径8mm,承重256公斤，技术参数：C碳≤0.08，镍8.11%，磷0.035%，硫≤0.03%，锰≤2.0%，不锈钢晾衣绳8mm，304不锈钢挂钩，304锈钢拉紧器。","米",1000]
[4,"不锈钢晾衣杆","工作内容：人工安装；参数：材质不锈钢，厚度0.8mm，直径2.5cm，含安装件1套（不锈钢座2个）。","根",450]
["四、寝室门维修更换"]
[5,"旧寝室门更换","工作内容：楼层搬运，安装辅料，人工安装，门框灌浆，门洞修复。","樘",50]
["六、卫生间及阳台防水补漏"]
[6,"卫生间及阳台防水补漏","工作内容：原卫生间阳台集成顶拆除恢复，室内补瓷粉，吸顶灯拆除恢复，卫生清理，管道疏通，注浆防水，垃圾清运，闭水实验。\n\n\n\n","间",10]
["七","合计"]
[null,"报价合计大写人民币：                                            元"]
["报价说明：1.本项目实行单价报价；2.表中报价数量预估数据参考，不作为结算依据，实际数量据实验收；3.报价包含所有税费。"]