{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["服务器清单"],"read":"whole","date_system":"1900"}

{"sheet":"服务器清单","index":0,"n_rows":7,"n_cols":8,"rows_kept":7,"merged":[[0,0,0,7],[1,0,1,7],[6,0,6,4]]}
["一卡通服务器采购及系统迁移服务服务报价表"]
["公司名称（印章）：                                                           联系人及电话：                         "]
["序号","名称","参数","数量","单位","单价","小计","备注"]
[1,"服务器","1.国内外知名厂商，2U机架式，标配原厂导轨；\n2.处理器：intel 4210R(2.4GHz/10核）处理器*2；\n3.内存：最大支持24根DDR4内存，配置128GB DDR4 RDIMM内存；\n4.硬盘：配置≥8个2.5寸热插拔硬盘槽位，可扩展至≥29个2.5寸热插拔硬盘槽位，同时可扩展2个3.5寸硬盘，且全部硬盘可在不打开主机箱盖的情况下热插拔维护，提供官网截图证明并加盖厂商鲜章；4块2.4TB 12G SAS 10K 2.5in EP 512e HDD通用硬盘模块；\n5.Raid卡：≥1个SAS RAID阵列卡，支持RAID0/1/10/5/6/50/60，4G缓存，含掉电保护；\n6.网卡：≥4个千兆网口，≥2个万兆光口（含光模块）；\n7.可配置≥3块双宽或8块单宽GPU卡，提供官方证明材料；\n8.电源及风扇：2*550W 交流&240V高压直流电源模块，支持热插拔冗余风扇；\n9.配置≥1Gb独立的远程管理控制端口；配置虚拟KVM功能,可实现与操作系统无关的远程对服务器的完全控制，包括远程的开机、关机、重启、更新Firmware、虚拟光驱、虚拟文件夹等操作，提供服务器健康日记、服务器控制台录屏/回放功能，能够提供电源监控，支持3D图形化的机箱内部温度拓扑图显示，可支持动态功率封顶，提供功能截图证明；\n10.支持外接USB WIFI模块，提供无线热点，用户可使用手机或便携机直接登录HDM，提供功能截图证明；\n11.支持OTP(One Time Password一次性密码)方案的双因素认证方案，提高系统安全性，提供功能截图证明；\n12.质保三年，并提供厂商售后服务承诺。",2,"台"]
[2,"阵列卡","940-8i  4GB缓存阵列卡",1,"块"]
[3,"系统迁移服务",null,1,"项"]
["合计："]