{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":9,"rows_kept":10,"merged":[[0,0,0,8],[9,2,9,8]]}
["毕节市第二届职业技能大赛“汽车维修”项目设备及技术服务租赁报价清单"]
["序号","服务及设备","租赁时间（天）","数量","单位","单价（元）","总价（元）","主要参数","备注"]
[1,"省赛国赛车型",7,2,"辆",null,null,"（一）产品功能\n1.整车具备完整的动力、制动、传动、转向、行驶、电气、空调及控制系统，各种工况正常，可以正常启动、行驶、制动。能够通过诊断电脑执行读取车辆信息、读取故障代码、数据流、执行元件测试等操作。\n2.整车有效地支撑了车辆认知、大赛训练、维修保养、整车拆装、故障检测等教学需求。\n（二）整车技术参数\n发动机：≥2.0T L4 ；排量(mL)：≥1984 \n最大功率(kW)：≥162 ；最大马力(PS)：≥220 \n最大功率转速(rpm)：≥4500-6200 \n最大扭矩(N·m)：≥350 \n进气形式：涡轮增压  ；变速箱：7挡湿式双离合 \n长×宽×高(mm)：≥4865×1832×1471 \n轴距(mm)：≥2871 \n主动安全配置：ABS防抱死、牵引力控制(ASR/TCS/TRC)、刹车辅助(EBA/BAS/BA)、并线辅助、车道偏离预警系统、车道保持辅助系统、主动刹车/主动安全系统、道路交通标示识别、疲劳驾驶提示、全速自适应巡航、远近光灯光源：LED、感应雨刷。\n多媒体配置：9.2寸中控台大屏、手机互联/映射（CarPlay、CarLife）、语音识别控制系统（多媒体系统、导航、电话）。"]
[2,"整车故障设置系统",7,2,"套",null,null,"1.检测模块总成数量：4块；J623部分测量面板，180个测量针脚；J519/J386/J387部分测量面板，180个测量针脚；J533部分测量面板，20个测量针脚；J965部分测量面板，40个测量针脚；\n2.6条测量连接线束，涵盖发动机控制单元J623、车载电网控制单元J519、左前车门控制单元J386、右前车门控制单元J387、进入及启动许可系统J965、网关J533。\n3.设备电源：DC12V\n4.工作温度约：-40℃ - +50℃\n5. 外形尺寸约：≥920*260*600mm（长*宽*高）","与比赛车型适配"]
[3,"万用接线盒（含4条Y型专用连接线）",7,2,"套",{"$nulls":3},"与比赛车型适配"]
[4,"示波器",7,2,"套",{"$nulls":3},"与比赛车型适配"]
[5,"集成工具管理车",7,2,"台",{"$nulls":3},"与比赛车型适配"]
[6,"适配工具",7,2,"套",{"$nulls":3},"与比赛车型适配"]
[7,"诊断仪",7,2,"台",{"$nulls":3},"与比赛车型适配"]
[8,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}