{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":9,"rows_kept":11,"merged":[[0,0,0,8],[10,2,10,8]]}
["毕节市第二届职业技能大赛“新能源汽车智能化技术”项目设备及技术服务租赁报价清单"]
["序号","服务及设备","租赁时间（天）","数量","单位","单价（元）","小计（元）","设备参数","备注"]
[1,"新能源国赛省赛车型",7,1,"辆",null,null,"（一）产品功能\n1.车辆各种工况正常，可以启动、行驶、各系统功能操作等；能够通过原厂诊断电脑与诊断座，读取车辆信息、编码查询、读取故障代码、高压数据流、执行元件测试等测试功能，真实贴近维修一线的工作和内容。\n2.基于整车的高压维修可以真实反映诊断维修状态，并且标准实施诊断维修过程时需要对高压系统进行高压警示线、高压警示牌的放置，表现维修专业度和高压安全意识。\n3.为保证设备高效运行，电池管理系统（BMS），交流充电单元（OBC），电机控制器（JX1）直接进行专用外接设计，通过无损连接，可实现快速测量诊断模块更换。\n（二）产品规格参数\n续航里程：550km\n电池容量：84.8KWh\n电机功率：150KW\n最大扭矩：310N·m\n车辆尺寸：4592×1852×1629MM\n轴距：2765MM\n电池类型：三元锂电池\n电机类型：永磁同步电机\n驾驶辅助系统：车道偏离预警系统、车道保持辅助系统、道路交通标示识别、主动刹车/主动安全系统、全速自适应巡航系统、自动驻车等。"]
[2,"整车故障设置系统平台",7,1,"套",null,null,"（一）产品功能\n1. 整车故障设置平台和故障检测盒以整车为基础，在不破坏原车电路情况下，可以轻松的串联在控制模块和原车线束之间。整车各控制系统、传感器、执行器功能齐全，可正常运行。\n2. 整车故障设置平台支持车辆电池管理系统、电机控制器、交流充电单元、无钥匙进入系统、车身控制系统、车身电气系统，网关，车门电脑部分的信号测量与故障设置。\n3.检测盒背面部分为机械故障设置终端，采用隐藏式机械故障设置系统，通过U型连接端子可设置断路、短路、偶发、接触不良、CAN线反接故障。\n4.检测盒前面部分为学生测量部分，可直接用万用表、示波器在面板上实时测量电压、电流、电阻、频率、波形信号等。\n（二）技术参数\n1.检测盒外形尺寸：920*270*600mm（长*宽*高）\n2.设备电源：DC12V\n3.工作温度：-40℃ - +50℃","与比赛车型匹配"]
[3,"解码器",7,1,"套",{"$nulls":3},"与比赛车型匹配"]
[4,"示波器",7,1,"套",{"$nulls":3},"与比赛车型匹配"]
[5,"一体工具管理车",7,1,"台",{"$nulls":3},"与比赛车型匹配"]
[6,"万用接线盒",7,1,"套",{"$nulls":3},"与比赛车型匹配"]
[7,"绝缘测试仪",7,1,"台",{"$nulls":3},"与比赛车型匹配"]
[8,"安全防护套装（包括人员套装和地面套装）",7,2,"套"]
[9,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}