{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":7,"rows_kept":6,"merged":[[0,0,0,6],[4,0,4,6]],"flags":["formulas_cached_only"]}
["毕节工业职业技术学院\n虚拟仿真实训室场地简易装修报价单"]
["序号","项目名称","规格型号","工程量","单价（元）","金额（元）","做法要求"]
[1,"地砖施工","800mm×800mm","1155㎡",null,null,"1.地砖：品质为通体釉面砖，优等品，表面平整、边角整齐，无裂纹、缺棱掉角等缺陷；外观颜色须与我校智慧校园建设及服务项目（一期）所用的地砖颜色一致，品种规格及物理性能符国家现行标准有关规定，有产品合格证明书及性能检测报告。\n2.水泥：硅酸盐水泥、普通硅酸盐水泥或矿渣水泥，其强度等级不应小于32.5，严禁不同品种、不同等级的水泥混用，水泥进场应有出厂合格证明书和检测报告，进场后应进行取样复试。其质量必须符合现行国家标准《硅酸盐水泥、普通硅酸盐水泥》的规定。当对水泥质量有怀疑或水泥出场超过三个月时，在使用前必须进行复试，并按复试结果使用。\n3.砂：中砂或粗砂，过5mm孔径筛子，其含泥量不大于3%。其质量应符合国家现行标准JGJ52—1992《普通混凝土用砂质量标准及检验方法》的规定。\n"]
[2,"踢脚线施工","800mm×100mm","370m",null,null,"1.地砖同等材质加工。\n2.如本项目总价报价相同，暗线安装方式优先中标。"]
["注：项目实施过程要做好成品保护工作，项目完工后须对损坏的成品进行免费修复。"]
["报价单位（盖章）：",{"$nulls":4},"联系人及联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}